FFmpeg commands:

     -pix_fmt rgb24                     //for RGB formats
     -pix_fmt yuv420p                   //for YUV formats
     -pix_fmt bgr24                     //for BGR formats

     -compression_algo raw              //for uncompressed


     -vf      "scale=4096:2160"         //scaling the resolution
               "crop=3840:2160:0:0"     //to cut the sice


     -framerate 60                      //for fps (frames per second)


     -vcodec libx264                    //for H264 Codec
     -vcodec libx265                    //for H265 Codec
     -vcodec prores_ks                  //for Prores
     -vcodec hap -format hap            /for HAP
     -vcodec hap -format hap_q          //for HAPQ

     - chunks 8                         //for hap: encoding can use 0-8 threads

     - vcodec prores -profile:v 2       //Prores Profiles: 
                                        //0: ProRes422 (Proxy) – apco
                                        //1: ProRes422 (LT) – apcs
                                        //2: ProRes422 (Normal) – apcn
                                        //3: ProRes422 (HQ)- apch
                                   
     -qscale:v 10                       // quality for prores 0-32 (9-13 good)

     -crf 24                            //value for the biterate when using H265 or H264 
                                        //CRF (Constant Rate Factory 0-51) small value --> high bitrate (22-26 is default)
     -preset veryslow                   //slow presets => better compression (veryslow,slow,fast,veryfast)

     %05d.tif                           //for picture sequences (decimal place) (image_00001.tif = image_%05d.tif)                    

     

endings:

     H265     = .mp4
     H264     = .mp4
     HAP      = .mov
     HAPQ     = .mov


Examples (flat video):
=======================



     TIFF --> DPX + scaling
     ffmpeg -i "V:\Frames_8kx4k\Testvideo_8192x4302_%04d.tif" -pix_fmt rgb24 -vf "scale=4096:2160" "V:\DPX 4096x2160 8Bit 60fps\RAW_DEMO_4k_8Bit_%04d.dpx"

     TIFF --> H264 420
     ffmpeg  -r 60 -i "V:\TIFF 4096x2160 16Bit 30fps\Testvideo_%05d.tif" -vcodec libx264 -r 60 -crf 26 -pix_fmt yuv420p "V:\H264 4096x2160 8Bit 60fps\Testvideo_4k_30fps.mp4"


     PNG --> HAP
     ffmpeg -r 60 -i "V:\4k_png\Testvideo_000%05d.png" -vcodec hap -format hap -chunks 8 -r 60 "V:\HAP 4096x2160 8Bit 60fps\Testvideo_4K_hap.mov"


     TIFF --> Prores 444
     ffmpeg -r 60 -i "V:\TIFF 4096x2160 8Bit 60fps\Testvideo_%05d.tif" -vcodec prores -c:v prores_ks -profile:v 3 -qscale:v 15 -pix_fmt yuv444p10le -vf "scale=1920:1080" -r 60 "V:\Testvideo_FHD_prores_444_HQ(3)_q15.mov"

     TIFF --> TGA
     ffmpeg -framerate 60  -i "V:\TIFF 4096x2160 8Bit 60fps\Testvideo_4K_8Bit_%05d.tif" -coder "raw" -pix_fmt bgr24 -vf "scale=1920:1080" "V:\Testvideo_FHD_8Bit_%05d.tga"


     Split a 7680x2160 DPX sequnece into two 3840x2160 parts:
 
     CROP left Part:
     ffmpeg -i "V:\Testvideo_%05d.dpx" -filter:v "crop=3840:2160:0:0" "V:\Testvideo_crop_left_%05d.dpx"
 
     CROP right Part:
     ffmpeg -i "V:\Testvideo_%05d.dpx" -filter:v "crop=3840:2160:3840:0" "V:\Testvideo_crop_right_%05d.dpx"



Examples (fulldome):
=====================

     PNG --> HAP Domemaster 4K@30Hz (1 file)
     ffmpeg -r 30 -i "V:\FRAMES_4K\Dome_30fps_%05d.png" -vcodec hap -format hap -r 30 "V:\ENC_4K\Dome_4K_30fps.mov"


     PNG --> HAP Domemaster 6K@60Hz (2 files: top and bottom)
     ffmpeg -r 60 -i "V:\FRAMES_6K\Dome_60fps_%05d.png" -filter:v "crop=6000:3000:0:0" -vcodec hap -format hap -r 60 "V:\ENC_4K\Dome_6K_60fps_TOP.mov"
     ffmpeg -r 60 -i "V:\FRAMES_6K\Dome_60fps_%05d.png" -filter:v "crop=6000:3000:0:3000" -vcodec hap -format hap -r 60 "V:\ENC_4K\Dome_6K_60fps_BOT.mov"


